|  |  |
| --- | --- |
| EAN 5901804422577 | CB NUMBER 3610  |
| Vendor Art. Number  |  |

**EASY ONE**

# Main description

The Easy is an all-electric towel rail enriched by the built-in One electric heating element. The heating element hidden in the Easy’s collector blends invisibly with its shape – without the need for an additional, external electric device. One is a practical and easy to use heating element which does not dominate the Easy radiator with its form. Easy owes its original look to a seamless connection between tubes and collectors. Simple, modern design can delight even the most demanding users.

# Key points

* All-electric towel rail
* Simple and modern design
* Easy hanging of the fabric to dry
* Functional built-in One electric heating element

# Features and benefits of the Easy radiator

* Highest quality low carbon steel ensuring product longevity
* Oxsilan® passive rust protection process
* High quality double layer powder coating
* 8 years warranty for water tightness and paint coating
* Increased resistance to chemicals, temperature variations and mechanical damage
* Easy cleaning and maintenance
* Easy installation (solid wall fixing kit included)
* Made to EN 10305-5

# Features and benefits of the One heating element

* Two operation modes: heating and drying
* TIMER function (automatically switches off the device after 2 hours)
* Ultra-low power consumption in standby mode (< 0,5 W)
* Device settings are remembered also after electricity cut-off, which makes it possible to work with external timers or intelligent building systems
* Option of adding extra functions by means of the built-in infrared link
* Protection against operation in dry conditions and double protection against radiator overheating
* Frost protection (ANTIFREEZE)

# Specifications

|  |  |
| --- | --- |
| Height (mm):  | 960 |
| Width (mm):  | 200 |
| Depth (mm):  | 70 |
| Colour:  | Sparkling gravel |
| Heat output (W):  | 200 |
| Heat output (BTUs): | 682 |
| Connection type:  | E8 |
| Connection spacing (mm): | N/A |
| Wall to centre of inlet (mm):  | N/A |
| Operating pressure (MPa):  | 0,8 |
| Maximum operating temperature (°C): | 60 |
| Material: | Carbon steel |
| Surface finish: | Powder coating |
| Weight (kg): | 7,25 |

Connection diagram

****

Sporządziła: Jagielska Magdalena 20170817

Poprawił: Danek Tomasz Terma Sp. z o.o. 2017-08-22