|  |  |
| --- | --- |
| EAN 5901804422638 | CB NUMBER 3522  |
| Vendor Art. Number  |  |

**QUADRUS BOLD**

# Main description

Modern design and functionality make this model ideal for any bathroom and kitchen. Quadrus Bold features a double row of flat tubes which give It good power output for its size.

The curved tube C and the space between the towel rail’s sections allow easy hanging of the fabric to dry.

# Key points

* Modern design
* High power output
* Easy hanging of the fabric to dry

# Features and benefits

* Highest quality low carbon steel ensuring product longevity
* Oxsilan® passive rust protection process
* High quality double layer powder coating
* Very good heat output
* 8 years warranty for water tightness and paint coating
* Increased resistance to chemicals, temperature variations and mechanical damage
* Easy cleaning and maintenance
* Easy installation (solid wall fixing kit included)
* Made to EN 10305-5

# Specifications

|  |  |
| --- | --- |
| Height (mm):  | 1185 |
| Width (mm):  | 450 |
| Depth (mm):  | 90 |
| Colour:  | Metallic Black |
| Heat output (W):  | 835 |
| Heat output (BTUs): | 2849 |
| Connection type:  | SX |
| Connection spacing (mm): | 420 |
| Wall to centre of inlet (mm):  | 57-65  |
| Operating pressure (MPa):  | 1 |
| Maximum operating temperature (°C): | 95 |
| Material: | Carbon steel |
| Surface finish: | Powder coating |
| Weight (kg): | 23,02 |

Connection diagram

****

Sporządziła: Jagielska Magdalena 20170817

Poprawił: Danek Tomasz Terma Sp. z o.o. 2017-08-22