|  |  |
| --- | --- |
| EAN 5901804191060 | CB NUMBER T1201 |
| Vendor Art. Nr 1804191060 |  |

SALISBURY

# Main description

Classic radiator distinguished by a functional arrangement of profiles, allowing easy access to towel rails. Can make a statement in any bathroom, kitchen or recreational space. Features robust rectangular profiles and a frame with rounded sides.

# Key points


* Simplicity and style
* High power output
* A form which is both minimalist and sophisticated
* Adheres very close to the wall

# Features and benefits

* Highest quality low carbon steel ensuring product longevity
* Excellent heat output
* Great towel hanging capability
* Every rail 100% leak tested
* Oxsilan® passive rust protection process
* High quality double layer powder coating
* Up to 8 Year Guarantee
* Increased resistance to chemicals, temperature variations and mechanical damage
* Easy installation (solid wall fixing kit included)
* Made to EN 10305-5
* Easy cleaning and maintenance

# Specifications

|  |  |
| --- | --- |
| Height (mm): | 1635 |
| Width (mm): | 540 |
| Depth (mm): | 40 |
| Colour: | Metallic Black |
| Heat output (W): | 794 |
| Heat output (BTUs): | 2709 |
| Connection type: | SX |
| Connection spacing (mm): | 500 |
| Wall to centre of inlet (mm): | 57-65 |
| Operating pressure (MPa): | 0.8 |
| Maximum operating temperature (°C): | 95 |
| Material: | Carbon steel |
| Surface finish: | Powder coating |
| Weight (kg): | 24.4 |

Connection diagram