|  |  |
| --- | --- |
| EAN 5901804422454 | CB NUMBER T3500 |
| Vendor Art. Number |  |

**ALEX**

# Main description

Simple and stylish. Ideally fits in both, classic and modern bathrooms and kitchens. The curved tube C and the space between the towel rail’s sections allow easy hanging of the fabric to dry.

# Key points

* Classic design
* Easy hanging of the fabric to dry

# Features and benefits

* Highest quality low carbon steel ensuring product longevity
* Oxsilan® passive rust protection process
* High quality double layer powder coating
* 8 years warranty for water tightness and paint coating
* Increased resistance to chemicals, temperature variations and mechanical damage
* Easy cleaning and maintenance
* Easy installation (solid wall fixing kit included)
* Made to EN 10305-5

# Specifications

|  |  |
| --- | --- |
| Height (mm): | 760 |
| Width (mm): | 500 |
| Depth (mm): | 100 |
| Colour: | Modern Grey |
| Heat output (W): | 412 |
| Heat output (BTUs): | 1406 |
| Connection type: | SX |
| Connection spacing (mm): | 470 |
| Wall to centre of inlet (mm): | 57 - 65 |
| Operating pressure (MPa): | 1 |
| Maximum operating temperature (°C): | 95 |
| Material: | Carbon steel |
| Surface finish: | Powder coating |
| Weight (kg): | 8,36 |

Connection diagram

****

Sporządziła: Jagielska Magdalena 20170817

Poprawił: Danek Tomasz Terma Sp. z o.o. 2017-08-22