|  |  |
| --- | --- |
| EAN 5901804422515 | CB NUMBER T3511  |
| Vendor Art. Number  |  |

**EASY**

# Main description

Easy owes its original look to a seamless connection between tubes and collectors. Simple, modern design can delight even the most demanding users and due to its petite size, fit in the smallest of bathrooms.

# Key points

* Simple and modern design
* Fits small bathrooms
* Easy hanging of the fabric to dry

# Features and benefits

* Highest quality low carbon steel ensuring product longevity
* Oxsilan® passive rust protection process
* High quality double layer powder coating
* 8 years warranty for water tightness and paint coating
* Increased resistance to chemicals, temperature variations and mechanical damage
* Easy cleaning and maintenance
* Easy installation (solid wall fixing kit included)
* Made to EN 10305-5

# Specifications

|  |  |
| --- | --- |
| Height (mm):  | 1280 |
| Width (mm):  | 200 |
| Depth (mm):  | 40 |
| Colour:  | Sparkling Gravel |
| Heat output (W):  | 251 |
| Heat output (BTUs): | 856 |
| Connection type:  | SX |
| Connection spacing (mm): | 160 |
| Wall to centre of inlet (mm):  | 57 – 65  |
| Operating pressure (MPa):  | 0,8 |
| Maximum operating temperature (°C): | 95 |
| Material: | Carbon steel |
| Surface finish: | Powder coating |
| Weight (kg): | 6,71 |

Connection diagram

****

Sporządziła: Jagielska Magdalena 20170817

Poprawił: Danek Tomasz Terma Sp. z o.o. 2017-08-22