|  |  |
| --- | --- |
| EAN 5901804191244 | CB NUMBER T1800 |
| Vendor Art. Nr 1804191244 |  |

JADE

# Main description

The classic towel rail. Wide gaps between profile sections make it a functional dryer. Jade can become an inconspicuous decorative feature of each room.

# Key points

* Modern design
* Functional and light towel rail
* Easy access to clothes and towels

# Features and benefits

* Highest quality low carbon steel ensuring product longevity
* Every rail 100% leak tested
* Hand polished surface ensuring state-of-the-art galvanic coating
* Great towel hanging capability
* Easy installation (solid wall fixing kit included)
* Easy cleaning and maintenance
* Made to EN 10305-5
* Bleed valve included

# Specifications

|  |  |
| --- | --- |
| Height (mm):  | 753 |
| Width (mm):  | 400 |
| Depth (mm):  | 61 |
| Colour:  | Galvanic Old Copper |
| Heat output (W):  | 174 |
| Heat output (BTUs): | 594 |
| Connection type:  | SX |
| Connection spacing: | 364 |
| Wall to centre of inlet (mm):  | 52-72 |
| Operating pressure (MPa):  | 1 |
| Maximum operating temperature (°C): | 95 |
| Material: | Carbon steel |
| Surface finish: | Galvanic coating |
| Weight (kg): | 4.4 |

Connection diagram