|  |  |
| --- | --- |
| EAN 5901804191107 | CB NUMBER T1401 |
| Vendor Art. Nr 1804191107 |  |

RETRO

# Main description

The form of this radiator cannot be confused with any other model. It makes a statement in various types of space – not only in rustic or old-style interiors – adding character and style.

# Key points

* Retro style radiator with uncommon profiles and valves
* Unique form and finish
* Wide spaces between profiles make it easy to hang clothes

# Features and benefits

* Highest quality low carbon steel ensuring product longevity
* Easy installation (solid wall fixing kit included)
* Every rail 100% leak tested
* Hand polished surface ensuring state-of-the-art galvanic coating
* Great towel hanging capability
* Bleed valve included
* Made to EN 10305-5

# Specifications

|  |  |
| --- | --- |
| Height (mm):  | 1170 |
| Width (mm):  | 504 |
| Depth (mm):  | 65 |
| Colour:  | Galvanic Old Copper |
| Heat output (W):  | 216 |
| Heat output (BTUs): | 737 |
| Connection type:  | SX |
| Connection spacing: | 450 |
| Wall to centre of inlet (mm):  | 39-49 |
| Operating pressure (MPa):  | 1 |
| Maximum operating temperature (°C): | 95 |
| Material: | Carbon steel |
| Surface finish: | Galvanic coating |
| Weight (kg): | 10.2 |

Connection diagram