|  |  |
| --- | --- |
| EAN 5901804191367 | OPCO NUMBER T2004 |
| Vendor Art. Nr 1804191367 |  |

Swale

# Main description

New technologies allow radiator designers to introduce new and uncommon forms. Original design, highest quality and functionality make Swale a great choice not only for bathrooms, but also for other spaces in modern interiors.

# Key points

* Unique asymmetric form
* Original and functional decorative element
* Ultimate minimalism and practical value

# Features and benefits

* Highest quality low carbon steel ensuring product longevity
* Every rail 100% leak tested
* Oxsilan® passive rust protection process
* Great towel hanging capability
* High quality double layer powder coating
* Up to 8 Year Guarantee
* Increased resistance to chemicals, temperature variations and mechanical damage
* Easy installation (solid wall fixing kit included)
* Easy cleaning and maintenance
* Made to EN 10305-5
* Bleed valve included

# Specifications

|  |  |
| --- | --- |
| Height (mm):  | 1200 |
| Width (mm):  | 465 |
| Depth (mm):  | 32 |
| Colour:  | Metallic Black |
| Heat output (W):  | 757 |
| Heat output (BTUs): | 2583 |
| Connection type:  | YP |
| Connection spacing: | 50 |
| Wall to centre of inlet (mm):  | 67-75 |
| Operating pressure (MPa):  | 1 |
| Maximum operating temperature (°C): | 95 |
| Material: | Carbon steel |
| Surface finish: | Powder coating |
| Weight (kg): | 13 |

Connection diagram